SECTION 1.06 CONTROL OF MATERIALS

Article 1.06.01 ‑ Source of Supply and Quality:

Add the following:

**Traffic Signal Items:**

For the following traffic signal items the contractor shall submit a complete description of the item, shop drawings, product data sheets and other descriptive literature which completely illustrates such items presented for formal review. Such review shall not change the requirements for a certified test report and materials certificate as may be called for. All documents shall be grouped into one separate file for each group of items as indicated by the Roman numerals below (for example, one pdf file for all of the pedestal items). The documents for all of the traffic signal items shall be submitted at one time, unless otherwise allowed by the engineer.

1. 1003206 – Light Standard (15' Bracket, 30' Mounting Height)
2. 10080XX – Rigid Metal Conduit

1013008 – 1 ¼" Liquid Tight Flexible Metal Conduit

1017032 – Service (Metered) Slip Fitting

1. 11020XX – Aluminum Pedestals
2. 11050XXA – Traffic Signals, Span Mounted - LEDs, Housings and Hardware

11051XXA – Traffic Signals, Mast Arm Mounted - LEDs, Housings and Hardware

11052XXA – Traffic Signals, Pole Mounted - LEDs, Housings and Hardware

11053XXA – Traffic Signals, Pedestal Mounted - LEDs, Housings and Hardware

11055XXA – LED Traffic Signal Lamp Unit

1. 1105503A – Flasher Cabinet
2. 11060XXA – Pedestrian Signals - LEDs, Housings, and Hardware

11070XXA – Pedestrian Pushbutton & Sign - Button, Housings & Sign (Type)

11070XXA – Accessible Pedestrian Signal & Detector - Button, Housings & Sign (Type)

1. 1108115A – Full Actuated Controller, 8-Phase – Cabinet and Components
2. 11XXXXXA – Optical Pre-Emption - Emitter, Detector, Phase Selector and Chassis

1114201A – Auxiliary Equipment Cabinet

1. 11XXXXXA – Siren pre-emption - Detector, Phase Selector and Confirmation Light
2. 11114XXA – Loop Detector Amplifier, Sealant, Wire and Lead in Wire
3. 11122XXA – Vehicle Detection - Camera Assembly, Processor and Monitor
4. 111339XA – Cable closure (Type)
5. 1113XXXA – Cable - Control Cable, Comm., CAT6, VC, Detector Cable (optical)

11134XXA – Control Cable – Communication Interconnect

1114101 – Messenger Wire

1. 1117101A – Alternate Flashing Signals for Warning Signs

111711XA – Rectangular Rapid Flashing Beacon